>> MIB - Management Information Base
>> Table: efmStatsTable - (.1.3.6.1.4.1.272.4.30.2.1.1)
Description: An entry in efmStatsTable.
efmStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Channel | INTEGER | R
.3 | InPkts | Counter64 | R
.4 | OutPkts | Counter64 | R
.5 | InOctets | Counter64 | R
.6 | OutOctets | Counter64 | R
.7 | InDiscards | Counter64 | R
.8 | OutDiscards | Counter64 | R
.9 | InErrors | Counter64 | R
IfIndex
Specifies the DSL interface index used on this line.
Channel
Specifies the QOS channel that is described in this entry.
InPkts
The number of reassembled received packets.
OutPkts
This number of transmitted packets.
InOctets
The total number of octets received on the interface, including framing characters.
OutOctets
The total number of octets transmitted out of the interface, including framing characters.
InDiscards
The number of inbound packets which were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol. One possible reason for discarding such a packet could be to free up buffer space.
OutDiscards
The number of outbound packets which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a packet could be to free up buffer space.
InErrors
The number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH