>> MIB - Management Information Base
>> Table: x25 - (.1.3.6.1.4.1.272.4.6)
x25
OID | Name | Type | Access
.10 | LocalPadCall | ENUM | RW
.11 | LocalAddr | DisplayString | RW
.12 | Rerouting | ENUM | RW
.13 | HistoryMaxEntries | INTEGER | RW
.14 | AccountingTemplate | DisplayString | RW
LocalPadCall
This object specifies wether a PAD Call (PID=1) routed to the local X.25 entity (ifIndex=1) should be accepted to allow for a remote login via X.25. This may be disabled for security reasons by setting this object do dont-accept. Enumerations: accept (1) dont-accept (2)
LocalAddr
The X.25 address to be used as originating address for outgoing X.25 call from this BRICK. A leading @ indicates extended adressing. Length: 0 to 255
Rerouting
This object specifies whether a rerouting request should be accepted to establish connection to another server. This is only relevant for x29 rerouting. Enumerations: allow (1) disallow (2)
HistoryMaxEntries
Maximum number of x25CallHistory entries in memory. Range: 0 to 255
AccountingTemplate
Specifies the format of accounting messages sent by the syslog protocol. The format can consist of any order of the following variables. Tag Meaning %S Date and Time the connection was established; in DD.MM.YY/HH:MM:SS format. %d The duration of the connection in seconds. %z The X25 source address. %Z The X25 destination address. %y Total number of bytes received over the connection. %Y Total number of bytes sent over the connection. %g Total packets received over the connection. %G Total packets sent over the connection. %c The X25 clear cause. %C The X25 clear diagnostic. %f The source interface. %F The destination interface. %v The source virtual channel number. %V The destination virtual channel number. The default accounting template setting contains the following tags: %S,%d,%z,%Z,%y,%Y,%g,%G,%c,%C. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH