>> MIB - Management Information Base
>> Table: dot1dBase - (.1.3.6.1.4.1.272.4.8.1)
dot1dBase
OID | Name | Type | Access
.1 | BridgeAddress | MacAddress | R
.2 | NumPorts | INTEGER | R
.3 | Type | ENUM | R
BridgeAddress
The MAC address used by the BRICK when it must be referred to in a unique fashion. It is recommended that this be the numerically smallest MAC address of all ports belonging to the BRICK. However it is only required to be unique. When concatenated with dot1dStpPriority a unique BridgeIdentifier is formed which is used in the Spanning Tree Protocol. Length: 6 to 6
NumPorts
The number of ports controlled by the BRICK.
Type
Indicates what type of bridging this BRICK can perform. If the BRICK is actually performing a certain type of bridging this will be indicated by entries in the port table for the given type. Enumerations: unknown (1) transparent-only (2) sourceroute-only (3) srt (4)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH