>> MIB - Management Information Base
>> Table: ospfIfMetricTable - (.1.3.6.1.2.1.14.8.1)
Description: A particular TOS metric for a non-virtual interface identified by the interface index.
ospfIfMetricTable
OID | Name | Type | Access
.1 | IpAddress | IpAddress | R
.2 | AddressLessIf | INTEGER | R
.3 | TOS | INTEGER | R
.4 | Value | INTEGER | RW
.5 | Status | ENUM | R
IpAddress
The IP address of this OSPF interface. On row creation, this can be derived from the instance.
AddressLessIf
For the purpose of easing the instancing of addressed and addressless interfaces; This variable takes the value 0 on interfaces with IP Addresses, and the value of ifIndex for interfaces having no IP Address. On row creation, this can be derived from the instance.
TOS
The type of service metric being referenced. On row creation, this can be derived from the instance. Range: 0 to 31
Value
The metric of using this type of service on this interface. The default value of the TOS 0 Metric is 10^8 / ifSpeed. The value FFFF is distinguished to mean 'no route via this TOS'. Range: 1 to 65535
Status
This variable displays the validity or invalidity of the entry. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH