>> MIB - Management Information Base
>> Table: voipStatRtcpTable - (.1.3.6.1.4.1.272.4.33.22.3.1)
Description: Describes current call specific statistics calculated from RTCP contents
voipStatRtcpTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Reference | INTEGER | R
.3 | Duration | TimeStamp | R
.4 | RoundTripDelay | INTEGER | R
.5 | AvgRoundTripDelay | INTEGER | R
.6 | LocalIdent | DisplayString | R
.7 | LocalInterarrivalJitter | INTEGER | R
.8 | LocalAvgInterarrivalJitter | INTEGER | R
.9 | LocalPackets | Counter32 | R
.10 | LocalBytes | Counter32 | R
.11 | LocalPacketLossRate | INTEGER | R
.12 | RemoteIdent | DisplayString | R
.13 | RemoteInterarrivalJitter | INTEGER | R
.14 | RemoteAvgInterarrivalJitter | INTEGER | R
.15 | RemotePackets | Counter32 | R
.16 | RemoteBytes | Counter32 | R
.17 | RemotePacketLossRate | INTEGER | R
Index
Unique Index to reference this call
Reference
Reference to the Account the local statistic belongs.
Duration
The Duration of the current call.
RoundTripDelay
Current round trip delay in microseconds calculated as defined in [Section6.4/RFC3550].
AvgRoundTripDelay
Average round trip delay in microseconds since the beginning of the current call. Average of the RoundTripDelay statistic accumulated each time the delay is calculated.
LocalIdent
Current Local Source Description transfered in SDES defined in [Section6.5/RFC3550]. Length: 0 to 255
LocalInterarrivalJitter
Current receive interarrival jitter in microseconds. Calculated from J(i) as defined in [Section6.4/RFC3550], with units converted to microseconds.
LocalAvgInterarrivalJitter
Average receive interarrival jitter in microseconds since the beginning of the current call. Calculated as the average of D(i,j) as defined in [Section6.4/RFC3550], with units converted to microseconds.
LocalPackets
Current count of local generated RTP data Packets for this call from DSP.
LocalBytes
Current count of local generated RTP data bytes for this call from DSP.
LocalPacketLossRate
Current receive packet loss rate in percent, calculated as defined in [Section6.4/RFC3550]. Range: 0 to 100
RemoteIdent
Current Source Description defined in [Section6.5/RFC3550] Length: 0 to 255
RemoteInterarrivalJitter
Current Interarrival jitter in microseconds as reported from the far-end device via RTCP. Calculated from J(i) as defined in [Section64./RFC3550], with units converted to microseconds.
RemoteAvgInterarrivalJitter
Average far-end interarrival jitter in microseconds since the beginning of the current call. Calculated as the average of the interarrival jitter values reported by the far-end, with units converted to microseconds.
RemotePackets
Current count of far-end generated RTP data Packets for this call from RTCP signalling.
RemoteBytes
Current count of far-end generated RTP data bytes for this call from RTCP signalling.
RemotePacketLossRate
Current far end receive packet lost rate in percent, calculated as defined in [Section6.4/RFC3550]. Range: 0 to 100

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH