>> MIB - Management Information Base
>> Table: serviceCallTable - (.1.3.6.1.4.1.272.4.22.8.2.1)
Description: Currently configured tunnels for service-call-feature. Normally, all entries share the same ticket-number, and there is one entry for the control-tunnel between service-call-daemon and server, and one entry per each to-be-tunnelled service-type.
serviceCallTable
OID | Name | Type | Access
.1 | Index | INTEGER | RC
.2 | OperStatus | ENUM | R
.3 | AdminStatus | ENUM | D
.4 | Type | ENUM | RW
.5 | ForwardedService | ENUM | RW
.6 | ForwardedIP | IpAddress | RW
.7 | Ticket | DisplayString | RC
.8 | Duration | TimeTicks | R
.9 | HostPort | INTEGER | R
.10 | UserId | DisplayString | R
Index
Internal identifier of this tunnel.
OperStatus
Current operational state of this tunnel. States relevant for forwarding-entries only: forward - Tunnelling/forwarding started. States relevant for control-entry only: register - Device-registration ongoing. ready - Ready for tunnel-requests from server. States relevant for all entry-types: new - Processing not yet started. connect - Connecting to server. login - Logging into server. blocked - Waiting for network to become available again. error - Processing aborted. Enumerations: new (7) connect (8) login (9) forward (10) register (11) ready (12) blocked (13) error (14)
AdminStatus
Activate/deactivate/delete this tunnel. Enumerations: enabled (1) disabled (2) delete (3)
Type
Type of target-unit accessed via this tunnel. (Implicitly always pbx for control-tunnel.) pbx - This PBX (or router) shall be accessed. phone - A phone attached to this PBX shall be accessed. Enumerations: pbx (1) phone (2)
ForwardedService
Type of to-be-tunnelled service for this entry. control - Control-tunnel between service-call-daemon and server. http - HTTP (port 80). https - HTTPS (using SSL, port 443). shell - Telnet (port 23). trace - Bricktrace for packet-capturing (port 7000). Enumerations: control (1) http (2) https (3) shell (4) trace (5)
ForwardedIP
For control-tunnel, two cases must be distinguished. For target-unit-type pbx, field is a dummy and may be set to 0.0.0.0. For target-unit-type phone, field is set to IP-address of phone. For service-tunnels, field is set to IP-address of target-unit (127.0.0.1 in pbx-case, and otherwise IP-address of phone).
Ticket
Ticket-number for this tunnel, to be copied to serviceCallUserId if not empty. Otherwise, derive serviceCallUserId from biboAdmSystemId. Length: 0 to 14
Duration
Duration of this tunnel.
HostPort
For control-tunnel, field is not relevant and is set to 0. For service-tunnels, field tells port-number dynamically allocated on called server for tunnelling this service via SSH-port-forwarding.
UserId
Temporary user-id for this tunnel (see also serviceCallTicket). Length: 0 to 14

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH