>> MIB - Management Information Base
>> Table: pimAnycastRPSetTable - (.1.3.6.1.4.1.272.4.5.54.2.1.12.1)
Description: An entry corresponds to a single router within a particular Anycast-RP set. This entry is preserved on agent restart.
pimAnycastRPSetTable
OID | Name | Type | Access
.1 | AddressType | ENUM | RC
.2 | AnycastAddress | InetAddressIPv6 | RC
.3 | RouterAddress | InetAddressIPv6 | RC
.4 | RowStatus | ENUM | D
.5 | LocalRouter | ENUM | R
AddressType
The address type of the Anycast-RP address and router address. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
AnycastAddress
The Anycast-RP address. The InetAddressType is given by the pimAnycastRPSetAddressType object. Length: 16 to 16
RouterAddress
The address of a router that is a member of the Anycast-RP set. The InetAddressType is given by the pimAnycastRPSetAddressType object. This address differs from pimAnycastRPSetAnycastAddress. Equal values for these two addresses in a single entry is not permitted. That would cause a Register loop. Length: 16 to 16
RowStatus
The status of this row, by which rows in this table can be created and destroyed. There are no other other writeable columnar objects in this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)
LocalRouter
Whether this entry corresponds to the local router. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH