>> MIB - Management Information Base
>> Table: phoneIfToneDefinitionTable - (.1.3.6.1.4.1.272.4.15.1.2.1)
Description: The phoneIfToneTable the contains configuration information for several tones on FXO and FXS lines.
phoneIfToneDefinitionTable
OID | Name | Type | Access
.1 | Index | ToneDefTabIndex | RW
.2 | Type | ENUM | RW
.3 | Freq1 | ToneFrequency | RW
.4 | Freq2 | ToneFrequency | RW
.5 | Level | INTEGER | RW
.6 | Cadence | CadenceString | RW
Index
Index of the set of tone cadences.
Type
Type of tone: single(1) just one frequency dual(2) mix of two frequencies Variables phoneIfToneDefinitionFreq1 and phoneIfToneDefinitionFreq2 specify frequencies involved as appropriate. Default value is single-tone. Enumerations: single (1) dual (2)
Freq1
Tone frequency 1: only tone (for single-tone type) or first tone of dual-tone signal (type dual-tone). Range: 300 to 3400
Freq2
Tone frequency 2: second tone of dual-tone signal. Ignored for single-tone entries. Range: 300 to 3400
Level
Tone signal level. Range: -50 to 0
Cadence
Cadence string for this single/dual-tone. The cadence definition consists of times of activity, times of no activity and some control information. All information is concatenated to one string and all times are given in milliseconds. Synopsis: [:] active time [:] [passive time] [:]... Arguments: active time a<time value in ms> passive time p<time value in ms> : start or end of loop interval ,|-|blank allowed delimiters for better reading before and behind the timing arguments Examples: 1) a200,p200,a200 => two tones with 200ms pause in between 2) a1000 p500 : a200 p200 : => a long pulse at the beginning followed by a continous interval of short pulses 3) p2000-a1000 => a pulse of one second after two second pause 4) :a1000: => definition for an endless active period Length: 0 to 127

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH