>> MIB - Management Information Base
>> Table: wlanPresence - (.1.3.6.1.4.1.272.4.46.35)
wlanPresence
OID | Name | Type | Access
.1 | Status | ENUM | RW
.2 | OperStatus | ENUM | R
.3 | OrgSecret | DisplayString | RW
.4 | CollectionInterval | INTEGER | RW
.5 | MaxElem | INTEGER | RW
.6 | DebugLevel | ENUM | RW
Status
Activates or deactivates the Presence Analytics daemon. Note that Presence Analytics must be enabled per-interface by means of 'wlanIfPresence' field.
OperStatus
Operational status of the daemon.
OrgSecret
Customer-specific secret. This secret is used to anonymize the client MAC addresses as part of the cryptographic mechanism.
CollectionInterval
The interval in seconds to contact the collection servers.
MaxElem
Maximum number of probes kept in memory. When the buffer is full, the oldest entry is deleted.
DebugLevel
Defines the verbosity of the debugging utility for this daemon. Level 'verbose' level shows the maximum amount of debugging information that can be generated by the daemon.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH