>> MIB - Management Information Base
>> Table: mpsCodecPropertyTable - (.1.3.6.1.4.1.272.4.53.8.2.1)
Description: This table contains information about codec properties referred by extensions and providers.
mpsCodecPropertyTable
OID | Name | Type | Access
.1 | Index | CodecIndex | RW
.2 | Descr | DisplayString | RW
.3 | Codecs | BitValue | RW
.4 | Order | ENUM | RW
.5 | Facilities | BITS | RW
.6 | AdminStatus | ENUM | D
Index
A unique value for each codec list. Range: 1 to 65535
Descr
Contains the description of codec property definition. Length: 0 to 20
Codecs
For codecs, supported by the provider or extension: ulaw (1) alaw (2) g729 (4) g726_24 (8) g726_16 (16) g726_32 (32) g726_40 (64) g728 (128) g723_63 (256) g723_53 (512) g729_e (1024) gsm (2048) dtmf (4096) g722 (8192) ilbc_13(16384) ilbc_15(32768) data (65536) Default ulaw, alaw, g.729 and dtmf. Range: 0 to -1
Order
Sorting the codecs default -> system default order quality -> highest quality first lowest -> lowest bandwith first highest -> highest bandwith first Enumerations: default (1) quality (2) lowest (3) highest (4)
Facilities
Facilities for codec settings: g726coding: 0 -> I.366 1 -> RFC 3551/X.420 avoidTranscoding: Use codec order of A call for B call on IP to IP calls independently of configured mpsCodecPropertyOrder. avoidAsymmetricCodecs: Answer with the same codec order as suggested by peer on hybrid calls independently of configured mpsCodecPropertyOrder. Enumerations: g726coding (1) avoidTranscoding (2) avoidAsymmetricCodecs (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH