>> MIB - Management Information Base
>> Table: mobileSmsSendTable - (.1.3.6.1.4.1.272.4.41.4.1.24.1)
Description: A single mobileSmsSendTable entry. This entry is temporary until it's successfully sent. After being successfully sent this entry is copied to the mobileSmsTable. Since the GSM/UMTS modem stores the SMS internally or on the SIM-Card this table is a NOSAVE table.
mobileSmsSendTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | IfIndex | INTEGER | RW
.3 | MsgStorage | ENUM | RW
.4 | MsgSlot | INTEGER | R
.5 | MsgStatus | ENUM | D
.6 | DestAddr | DisplayString | RW
.7 | MsgFormat | ENUM | RW
.8 | MsgCoding | ENUM | RW
.9 | MsgData | OCTET STRING | RW
Id
A unique ID generated by the application which triggers the SMS send request.
IfIndex
The interface index of the mobile device which should transmit the SMS.
MsgStorage
This object specifies the storage which holds the SMS. Available storages are: sm(1) -- SIM card storage me(2) -- Mobile Equipment storage The default of this object is 'me' because mobile equipment offers more storage normally. Enumerations: sm (1) me (2)
MsgSlot
The actual index to address the SMS in 'mobileSmsSendMsgStorage'. This index is returned by the mobile device after the store operation is successfully finished. Range: -1 to 65535
MsgStatus
The Status of the SMS. To start transmission of the SMS set Status to `transmit(1)'. On successful transmission the Status is set to `success(2)'. Afterwards the SMS is moved to the 'mobileSmsTable'. When transmission fails the Status changes to `error(3)'. The SMS stays in 'mobileSmsSendTable' for retransmissions. If the SMS should be deleted from the 'mobileSmsSendTable' and the mobile device storage specified in 'mobileSmsSendMsgStorage' the Status should be set to `delete(5)'. Enumerations: transmit (1) success (2) error (3) delete (5)
DestAddr
The destination address of this SMS. Length: 0 to 64
MsgFormat
The message format of the SMS. Traditional SMS use plain `txt(2)' format. Special or Unicode SMS use `pdu(1)' format. Enumerations: pdu (1) txt (2)
MsgCoding
This object specifies the coding of the SMS user data section. Enumerations: ira (1) gsm (2) ucs2 (3) pc437 (4) iso8859-1 (5)
MsgData
The raw text data of the SMS depending on the coding. Length: 0 to 160

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH