>> MIB - Management Information Base
>> Table: fsDiskTable - (.1.3.6.1.4.1.272.4.22.7.1.1)
Description: (one entry of fsDiskTable)
fsDiskTable
OID | Name | Type | Access
.1 | Id | INTEGER | R
.2 | DevName | DisplayString | R
.3 | DevInfo | DisplayString | R
.4 | Status | BITS | R
.5 | Command | ENUM | RW
.6 | FsType | ENUM | RW
.8 | Size | Unsigned32 | R
.9 | Blocks | Unsigned32 | R
.11 | FreeBlocks | Unsigned32 | R
.13 | InfoMsg | DisplayString | R
Id
Disk partition number. Directory path is /disk0..n Range: 0 to 255
DevName
Diskname and the alternative directory path. format: driver-devicenumber-partitionnumber e.g. ifl-0-0 (for internal flash device) Length: 0 to 32
DevInfo
Device hardware information. e.g. IN28F032 Length: 0 to 255
Status
Disk status flags Enumerations: inserted (0) mounted (1) readonly (2) error (7)
Command
Execute disk command mount: mount disk umount: umount disk to eject format: format whole disk (set together with FsType/Version) Enumerations: none (0) mount (1) umount (2) format (3)
FsType
Disk filesystem type. fat12 : FAT12 fat16 : FAT16 fat32 : FAT32 Enumerations: unkown (0) fat12 (1) fat16 (2) fat32 (3)
Size
Total disk size in kBytes.
Blocks
Number of disk/partition blocks (blocksize 512 bytes).
FreeBlocks
Number of free blocks.
InfoMsg
Last informational message. E.g. performed cmd message or occured error. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH