>> MIB - Management Information Base
>> Table: soipStatusTable - (.1.3.6.1.4.1.272.4.58.2.1)
Description: The soipStatusEntry contains status and statistic information of a SoIP interface.
soipStatusTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | UartRxBytes | Counter32 | R
.3 | UartTxBytes | Counter32 | R
.4 | UartRxParityErrors | Counter32 | R
.5 | UartRxOtherErrors | Counter32 | R
.6 | UartRxFifoErrors | Counter32 | R
.7 | UartSentXon | Counter32 | R
.8 | UartSentXoff | Counter32 | R
.9 | UartReceivedXon | Counter32 | R
.10 | UartReceivedXoff | Counter32 | R
.11 | IpRxBytes | Counter32 | R
.13 | IpTxBytes | Counter32 | R
.15 | IpRxFifoErrors | Counter32 | R
.16 | UartLocalHandshakeStatus | ENUM | R
.17 | UartRemoteHandshakeStatus | ENUM | R
.21 | IpStatus | ENUM | R
.22 | IpLocalIp | IpAddress | R
.23 | IpLocalPort | INTEGER | R
.24 | IpRemoteIp | IpAddress | R
.25 | IpRemotePort | INTEGER | R
Index
Reference to the concerned serial port.
UartRxBytes
Successful received bytes on the serial port.
UartTxBytes
Successful transmitted bytes on the serial port.
UartRxParityErrors
Receive parity errors on the serial port.
UartRxOtherErrors
Receive errors of all other types (framing, noise, ...) on the serial port.
UartRxFifoErrors
Receive buffer overflow on the serial port.
UartSentXon
XOn bytes sent by the local device on the serial port.
UartSentXoff
XOff bytes sent by the local device on the serial port.
UartReceivedXon
XOn bytes received from the remote device on the serial port.
UartReceivedXoff
XOff bytes received from the remote device on the serial port.
IpRxBytes
Successful received bytes via IP.
IpTxBytes
Successful transmitted bytes via IP.
IpRxFifoErrors
Receive buffer overflow on IP side.
UartLocalHandshakeStatus
Current local handshake status. on(1) -- receiving enabled off(2) -- receiving disabled Enumerations: on (1) off (2)
UartRemoteHandshakeStatus
Current remote handshake status. on(1) -- receiving enabled off(2) -- receiving disabled Enumerations: on (1) off (2)
IpStatus
Current connection status. not-connected(1) -- not connected connecting(2) -- connecting connected(3) -- connected conn-refused(4) -- connection refused peer-unreabable(5) -- peer unreachable peer-timeout(6) -- peer not answering (timeout) Enumerations: not-connected (1) connecting (2) connected (3) conn-refused (4) peer-unreabable (5) peer-timeout (6)
IpLocalIp
TCP server: Local IP. 0 = not connected. TCP client: Local IP. 0 = not connected. UDP unicast: Local IP packets get send from. UDP multicast: Local IP packets get send from.
IpLocalPort
TCP server: Local port. TCP client: Local port. UDP unicast: Local port packets get send from. UDP multicast: Local port packets get send from. Range: 0 to 65535
IpRemoteIp
TCP server: Remote IP. 0 = not connected. TCP client: Remote IP. 0 = not connected. UDP unicast: Remote IP the last packet was received from. UDP multicast: Remote IP the last packet was received from.
IpRemotePort
TCP server: Remote port. TCP client: Remote port. UDP unicast: Remote port the last packet was received from. UDP multicast: Remote port the last packet was received from. Range: 0 to 65535

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH