>> MIB - Management Information Base
>> Table: tr069Status - (.1.3.6.1.4.1.272.4.22.6.3)
tr069Status
OID | Name | Type | Access
.1 | StatusACSCommunication | ENUM | R
.2 | StatusACSCommSeqNo | Unsigned32 | R
.3 | StatusACSCommSeqNoLastMod | Unsigned32 | R
.4 | OperStatus | ENUM | R
.5 | OperStatusHint | DisplayString | R
.6 | StatusProductClass | DisplayString | R
.7 | StatusACSCommLastStart | Date | R
.8 | StatusACSCommLastEnd | Date | R
.9 | StatusACSCommLastSuccessfulStart | Date | R
.10 | StatusACSCommLastSuccessfulEnd | Date | R
.11 | StatusOutboundInterface | INTEGER | R
StatusACSCommunication
Indicate whether TR069 daemon is currently communicating with ACS. Value bocked means that communication is pending but can't be started due to an active configuration session. Enumerations: idle (1) running (2) blocked (3)
StatusACSCommSeqNo
Sequence number of current or last communication with ACS.
StatusACSCommSeqNoLastMod
Sequence number of last communication with ACS that resulted in a configuration change.
OperStatus
Show TR-069 operational status. this can be disabled although administrative status is enabled due to configuration settings that mustn't be revealed to TR-069 provider. Enumerations: disabled (1) enabled (2)
OperStatusHint
This variable holds descriptive information about operational status, e.g. why TR-069 is disabled despite being administratively enabled (in variable tr069Enabled). Length: 0 to 255
StatusProductClass
Product class the system conveys in InformationRequest message. This variable shows the effective product class as used in InformationRequest messages. See also variable tr069ProductClass. Length: 0 to 255
StatusACSCommLastStart
This variable contains the date when the last communication with ACS started. Range: 0 to -1
StatusACSCommLastEnd
This variable contains the date when the last communication with ACS started. Range: 0 to -1
StatusACSCommLastSuccessfulStart
This variable contains the date when the last communication with ACS started. Range: 0 to -1
StatusACSCommLastSuccessfulEnd
This variable contains the date when the last communication with ACS started. Range: 0 to -1
StatusOutboundInterface
This variable contains the outbound interface choosen when starting communication with the ACS.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH