>> MIB - Management Information Base
>> Table: ipRuleTable - (.1.3.6.1.4.1.272.4.5.16.1)
Description: The ipRuleTable defines access rules for checking incoming IP packets. The rules are processed in order, i.e. each rule has a link to the next rule. The set of rules is processed until a match occurs, that means the rule's associated filter matches and the specified action is performed (either accept or deny a packet). The last rule is implicitly a deny rule. The set of rules to be processed can be defined for each interface
ipRuleTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | FilterIndex | INTEGER | RW
.3 | Action | ENUM | D
.4 | NextRuleIndex | INTEGER | RW
.5 | Descr | DisplayString | RW
Index
Unique rule index.
FilterIndex
References the rule's associated filter.
Action
This object specifies the action to be performed if the rule's associated filter matches. If set to ignore the filter is not consulted and the next rule is processed immediately. Enumerations: allow (1) allow-if-not (2) deny (3) deny-if-not (4) ignore (5) delete (6)
NextRuleIndex
Specifies the next rule to be processed if the rule's associated filter does not match. The value 0 is used to mark the end of the rule set.
Descr
A textual string describing this access rule. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH