>> MIB - Management Information Base
>> Table: mpsVoIPConfig - (.1.3.6.1.4.1.272.4.53.8.3)
mpsVoIPConfig
OID | Name | Type | Access
.1 | ConfigRtpPort | INTEGER | RW
.2 | RegTimer | Unsigned32 | RW
.3 | DscpSignalling | INTEGER | RW
.4 | ServerCertIndex | INTEGER | RW
.5 | SubscribeTimer | Unsigned32 | RW
.6 | ConfigSipPort | INTEGER | RW
.7 | SupportedCodecs | BitValue | RW
.8 | ConfigSipNatPort | INTEGER | RW
.9 | ConfigIpVersion | ENUM | RW
ConfigRtpPort
Start value of dynamic RTP port.
RegTimer
Registration timer in seconds for IP extension. Set to 0 to get the time from the VoIP client.
DscpSignalling
The DSCP value used in IP header for signalling data. Range: 0 to 255
ServerCertIndex
Index of certificate entry in certTable to be used as server certificate for SIPS transport. If 0, predefined certificate of SIP stack is used.
SubscribeTimer
Timer value in seconds for SIP SUBSCRIBE session.
ConfigSipPort
Standard value of the SIP port.
SupportedCodecs
Bitmask for all codecs possibly supported by the system: ulaw (1) alaw (2) g729 (4) g726_24 (8) g726_16 (16) g726_32 (32) g726_40 (64) g728 (128) g723_63 (256) g723_53 (512) g729_e (1024) gsm (2048) dtmf (4096) g722 (8192) ilbc_13(16384) ilbc_15(32768) data (65536) System default: G.711ulaw, G.711alaw, G.729, G.726-32, G.722 and DTMF outband. Range: 0 to -1
ConfigSipNatPort
The external port mapped by NAT. For security reasons this might be different than the internal port (mpsVoIPConfigSipPort).
ConfigIpVersion
IP version used for VoIP communication. Enumerations: ipv4 (1) ipv4-ipv6 (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH