>> MIB - Management Information Base
>> Table: wlanVSSRateControlTable - (.1.3.6.1.4.1.272.4.46.37.1)
Description: Allows to modify the 'Rate Control' per VSS
wlanVSSRateControlTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Supported24Ghz | BITS | RW
.3 | Basic24Ghz | BITS | RW
.4 | Supported5Ghz | BITS | RW
.5 | Basic5Ghz | BITS | RW
IfIndex
Reference to the associated VSS entry.
Supported24Ghz
Defines the list in Mb/s of non-HT data rates at which the stations may transmit data in the 2,4 Ghz band.
Basic24Ghz
Defines the subset of the basic rates that are announced by the AP in the 2,4 Ghz band. For each basic rate, the corresponding supported rate must be present. The lowest value of this list will be used as the multicast and broadcast frame rates.
Supported5Ghz
Defines the list in Mb/s of non-HT data rates at which the stations may transmit data in the 5 Ghz band.
Basic5Ghz
Defines the subset of the basic rates that are announced by the AP in the 5 Ghz band. For each basic rate, the corresponding supported rate must be present. The lowest value of this list will be used as the multicast and broadcast frame rates.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH