>> MIB - Management Information Base
>> Table: mpsExtensionDiversionTable - (.1.3.6.1.4.1.272.4.53.6.9.1)
Description: This table contains the configured diversions.
mpsExtensionDiversionTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | Service | ENUM | RW
.3 | CFU | DisplayString | RW
.4 | CFB | DisplayString | RW
.5 | CFNR | DisplayString | RW
.6 | CFU2 | DisplayString | RW
.7 | CFU3 | DisplayString | RW
.8 | CFU3Fixed | ENUM | RW
.9 | CFU3Active | ENUM | RW
.10 | AdminStatus | ENUM | D
Index
A unique value for the extension, who has configured this diversion. Range: 1 to 65535
Service
Diversion for a special service. Enumerations: telephone (2) telephone3k1hz (3) telephoneAnalog (4) telephone7k1hz (5) analog (6) analogFaxG2 (7) analogFaxG3 (8) dataViaModem (9) btxViaModem (10) x21 (11) x21Uc4 (12) x21Uc5 (13) x21Uc6 (14) x21Uc19 (15) telefaxG4 (16) btx64kbit (17) data64kbit (18) x25 (19) x25Uc8 (20) x25Uc9 (21) x25Uc10 (22) x25Uc11 (23) x25Uc13 (24) x2519k2hz (25) teletex64 (26) mixedMode (27) telematicControl (28) grafiktelefondienste (29) btxNew (30) videoTelephone (31) videoTelephone3k1hz (32) videoTelephone7khz (33) videoTelephonePicture (34) speech (35) unrestrictedDigitalInformation (36) audio3k1 (37) audio7k (38) videotextInternational (39) allServices (40)
CFU
Destination number for call forwarding unconditional. Length: 0 to 24
CFB
Destination number for call forwarding busy. Length: 0 to 24
CFNR
Destination number for call forwarding no reply. Length: 0 to 24
CFU2
This variable contains the diversion target number for call deflection. Length: 0 to 24
CFU3
This variable contains the diversion target number for follow me. Length: 0 to 24
CFU3Fixed
This value determines whether the follow me diversion (CFU3) is fixed(1) or variable(2). Enumerations: true (1) false (2)
CFU3Active
This value determines whether the follow me diversion (CFU3) is active(1) or not active(2). Enumerations: true (1) false (2)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH