>> MIB - Management Information Base
>> Table: wlanLinkTestTable - (.1.3.6.1.4.1.272.4.46.11.1)
Description: An entry in WlanLinkTestEntry.
wlanLinkTestTable
OID | Name | Type | Access
.1 | SignalLocal | WlanRSSI | R
.2 | SignalRemote | WlanRSSI | R
.3 | NoiseLocal | WlanRSSI | R
.4 | NoiseRemote | WlanRSSI | R
.5 | SNRLocal | INTEGER | R
.6 | SNRRemote | INTEGER | R
.7 | FramesTransmitted | Counter32 | R
.8 | FramesReceived | Counter32 | R
.9 | FramesLost | Counter32 | R
.10 | RateLocal | WlanRate | R
.11 | RateRemote | WlanRate | R
.32 | RxFrames54 | Counter32 | R
.33 | RxFrames48 | Counter32 | R
.34 | RxFrames36 | Counter32 | R
.35 | RxFrames24 | Counter32 | R
.36 | RxFrames18 | Counter32 | R
.37 | RxFrames12 | Counter32 | R
.38 | RxFrames11 | Counter32 | R
.39 | RxFrames9 | Counter32 | R
.40 | RxFrames6 | Counter32 | R
.41 | RxFrames5 | Counter32 | R
.42 | RxFrames2 | Counter32 | R
.43 | RxFrames1 | Counter32 | R
.50 | Update | INTEGER | RW
.60 | RxFramesRemote54 | Counter32 | R
.61 | RxFramesRemote48 | Counter32 | R
.62 | RxFramesRemote36 | Counter32 | R
.63 | RxFramesRemote24 | Counter32 | R
.64 | RxFramesRemote18 | Counter32 | R
.65 | RxFramesRemote12 | Counter32 | R
.66 | RxFramesRemote11 | Counter32 | R
.67 | RxFramesRemote9 | Counter32 | R
.68 | RxFramesRemote6 | Counter32 | R
.69 | RxFramesRemote5 | Counter32 | R
.70 | RxFramesRemote2 | Counter32 | R
.71 | RxFramesRemote1 | Counter32 | R
.99 | IfIndex | INTEGER | R
SignalLocal
This attribute shows the received signal strength in dBm. Range: -110 to 0
SignalRemote
This attribute shows the received signal in dBm, as measured by remote bridge link partner. Reading this attribute triggers transmission of a new link request frame. Range: -110 to 0
NoiseLocal
This attribute shows the measured noise level in dBm. Range: -110 to 0
NoiseRemote
This attribute shows the noise level in dBm, as measured by remote bridge link partner. Range: -110 to 0
SNRLocal
This attribute shows the calculated Signal to Noise ratio in dB. Range: 0 to 90
SNRRemote
This attribute shows the calculated Signal to Noise ratio in dB, as measured by remote bridge link partner. Range: 0 to 90
FramesTransmitted
This attribute shows the number of link test frames transmitted.
FramesReceived
This attribute shows the number of link test frames successfully received.
FramesLost
This attribute shows the number of link test frames for which no reply has been received and therefore are considered lost.
RateLocal
This attribute shows the data rate of the most recent received link test frame, in 500 Kbps units. Range: 0 to 600
RateRemote
This attribute shows the data rate of the most recent link test frame received by the link partner, in 500 Kbps units. Range: 0 to 600
RxFrames54
This attribute shows the number of link test frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of link test frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of link test frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of link test frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of link test frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of link test frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of link test frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of link test frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of link test frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of link test frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of link test frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of link test frames that were received at 1 Mbps.
Update
Writing any non-zero value to this attribute triggers transmission of a new link request frame. Reading this attribute always returns 0.
RxFramesRemote54
This attribute shows the number of link test frames that were received by the remote partner at 54 Mbps.
RxFramesRemote48
This attribute shows the number of link test frames that were received by the remote partner at 48 Mbps.
RxFramesRemote36
This attribute shows the number of link test frames that were received by the remote partner at 36 Mbps.
RxFramesRemote24
This attribute shows the number of link test frames that were received by the remote partner at 24 Mbps.
RxFramesRemote18
This attribute shows the number of link test frames that were received by the remote partner at 18 Mbps.
RxFramesRemote12
This attribute shows the number of link test frames that were received by the remote partner at 12 Mbps.
RxFramesRemote11
This attribute shows the number of link test frames that were received by the remote partner at 11 Mbps.
RxFramesRemote9
This attribute shows the number of link test frames that were received by the remote partner at 9 Mbps.
RxFramesRemote6
This attribute shows the number of link test frames that were received by the remote partner at 6 Mbps.
RxFramesRemote5
This attribute shows the number of link test frames that were received by the remote partner at 5.5 Mbps.
RxFramesRemote2
This attribute shows the number of link test frames that were received by the remote partner at 2 Mbps.
RxFramesRemote1
This attribute shows the number of link test frames that were received by the remote partner at 1 Mbps.
IfIndex
Auxiliary index in wlanLinkTestTable.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH