>> MIB - Management Information Base
>> Table: ip6DhcpGenericOptTable - (.1.3.6.1.4.1.272.4.5.100.4.4.1)
Description: With this table, some stateless DHCPv6-options with fixed values can be specified rather generically. This may be useful for configuring such options that lack dedicated support by current DHCPv6-code and that may even be completely proprietary or vendor-specific. However, great care should be taken not to specify any options here that may interfere with any 'regular' ones, i.e. such that are automatically handled by current DHCPv6-code or that are configured by some dedicated, option-code-specific tables. At present, all (matching) configured generic options are put into related Advertise/Reply messages even if their option-codes have not been requested by Option Request Option (see 22.7 of RFC-3315). Each matching generic option results in a separate option-entry (in arbitrary order) even if sharing same option-code.
ip6DhcpGenericOptTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | Code | INTEGER | RW
.6 | Data | OCTET STRING | RW
Id
Internal identifier of this option-entry.
AdminStatus
Activate/deactivate/delete this option-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this option-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this option-entry is ignored. Range: 1 to 65535
Code
DHCPv6-option-code of this entry (see 22.1 of RFC-3315). Please read warning in general description of this table about not specifying any option-codes here that may interfere with 'regular' options-processing. Range: 0 to 65535
Data
Data-string that is pasted into data-part of this option-entry (see 22.1 of RFC-3315).

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH