>> MIB - Management Information Base
>> Table: ipWolRuleTable - (.1.3.6.1.4.1.272.4.5.67.1)
Description: The ipWolRuleTable defines access rules for checking incoming IP packets. The rules are processed in order, i.e. each rule has a link to the next rule. The set of rules is processed until a match occurs, that means the rule's associated filter matches and the specified action is performed (either send a Wake-On-LAN packet via Ethernet or via UDP). The last rule is implicitly a deny rule. The set of rules to be processed can be defined for each interface.
ipWolRuleTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | FilterIndex | INTEGER | RW
.3 | Action | ENUM | D
.4 | NextRuleIndex | INTEGER | RW
.5 | WolType | ENUM | RW
.6 | Target | MacAddress | RW
.7 | Password | DisplayString | RW
.8 | Descr | DisplayString | RW
.9 | TargetIfIndex | INTEGER | RW
Index
Unique rule index.
FilterIndex
References the rule's associated filter.
Action
This object specifies the action to be performed if the rule's associated filter matches. If set to ignore the filter is not consulted and the next rule is processed immediately. invoke, invoke WoL if filter matches invoke-if-not, invoke if filter not matches deny, deny WoL if filter matches deny-if-not, deny WoL if filter not matches ignore, ignore rule and skip to next rule delete delete the entry from the table Enumerations: invoke (1) invoke-if-not (2) deny (3) deny-if-not (4) ignore (5) delete (6)
NextRuleIndex
Specifies the next rule to be processed. The value 0 is used to mark the end of the rule set.
WolType
Which Wake-On-LAN standard should be used. Enumerations: ether (1) udp (2)
Target
The mac address of the interface to be woken up. Length: 6 to 6
Password
Wake-On-LAN password. The password length is either 0, 4 or 6. Length: 0 to 6
Descr
A textual string describing this Wake-On-LAN rule. Length: 0 to 255
TargetIfIndex
The index value which uniquely identifies Wake-On-LAN outbound interface.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH