>> MIB - Management Information Base
>> Table: biboDialTable - (.1.3.6.1.4.1.272.4.4.1.1)
Description: The biboDialTable contains configuration information for incoming and outgoing ISDN telephone numbers. Creating entries: Entries are created by assigning a value to the biboDialIfIndex object. Deleting entries: An entry can be removed by assigning the value `delete' to its biboDialType object.
biboDialTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Type | ENUM | D
.3 | Direction | ENUM | RW
.4 | Number | DisplayString | RW
.5 | Subaddress | OCTET STRING | RW
.6 | ClosedUserGroup | INTEGER | RW
.7 | StkMask | BitValue | RW
.8 | Screening | ENUM | RW
.9 | CallingSubaddress | OCTET STRING | RW
.10 | TypeOfCallingSubAdd | ENUM | RW
.11 | TypeOfCalledSubAdd | ENUM | RW
.12 | LocalNumber | DisplayString | RW
.13 | TypeOfLocalNumber | ENUM | RW
.14 | OutNumTranslation | ENUM | RW
IfIndex
The correlating PPP interface index.
Type
The dialup type can be set to plain isdn(1), isdn-spv(2) semi-permanent links used by the German 1TR6 D-channel protocol, or to delete(3) to delete a biboDialTable entry. The types ppp-callback(4) and ppp-negotiated(5) are used for the LCP callback option. Enumerations: isdn (1) isdn-spv (2) delete (3) ppp-callback (4) ppp-negotiated (5) x25-dialout (6) ip (7) x25 (8)
Direction
The allowed dial direction is either incoming(1), outgoing(2), or both(3) calls. No call is ever set up when set to incoming(1). Incoming calls will not be identified when set to outoing(2). Furthermore, once PPP authentication succeeds and there is at least one incoming number defined but for which none matches, the call will not be accepted for security reasons. Enumerations: incoming (1) outgoing (2) both (3)
Number
The defined dialing number. Used for either dialing or comparing to incoming calls or both, depending on the content of the biboDialDirection field. The wildcards '*', '?', '[', ']', '{', '}' may be used. Length: 0 to 63
Subaddress
The defined dial subaddress, if any. Also, see the biboDialNumber field.
ClosedUserGroup
The defined closed user group, if any. Also, see the biboDialNumber field. Range: 0 to 9999
StkMask
The defined stack mask. Each value of IsdnStkNumber represents a bit in this bitmask. A mask of 0 disables dialup completely, while a mask of -1 enables dialup on all available ISDN stacks. Range: 0 to -1
Screening
The screening indicator of the biboDialNumber. The biboDialScreening field can be used to gauge the `trustworthiness' of the biboDialNumber field. (See isdnCallScreening) Indicators are ordered from highest to lowest as follows: indicator: CPN assigned: verification: `network' by network none `user-verified' by user verification successful `user' by user none `user-failed' by user verification failed Set this field to `dont-care' to accept all calls. Otherwise calls are accepted only if the screening indicator matches or is higher than the set value. Enumerations: user (1) user-verified (2) user-failed (3) network (4) dont-care (5)
CallingSubaddress
The defined calling dial subaddress, if any. Also, see the biboDialNumber field.
TypeOfCallingSubAdd
The type of calling party subaddress. Enumerations: nsap (1) user-specified (2) reserved (3)
TypeOfCalledSubAdd
The type of called party subaddress. Enumerations: nsap (1) user-specified (2) reserved (3)
LocalNumber
The defined local dialing number. Used as originator address in the case of an outgoing calling and is checked against the destination address in the case of an incoming call. The wildcards '*', '?', '[', ']', '{', '}' may be used. Length: 0 to 63
TypeOfLocalNumber
The type of local number (biboDialLocalNumber) upon outgoing calls according to ETS 300 102-1. Possible values are: unknown(1), international-number(2), national-number(3), network-specific-number(4), subscriber-number(5) Default value is unknown. Enumerations: unknown (1) international-number (2) national-number (3) network-specific-number (4) subscriber-number (5)
OutNumTranslation
If DialOutNumTranslation is disabled, the number will be passed to the lower layers without modification. Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH