>> MIB - Management Information Base
>> Table: systemPhoneOemUserTable - (.1.3.6.1.4.1.272.4.64.6.2.1)
Description: This table contains personal information about OEM system phones. (It must be autosaved because the parameter can be changed by a user).
systemPhoneOemUserTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | Language | ENUM | RW
.3 | AdminStatus | ENUM | D
.4 | AutoCallAccept | ENUM | RW
Index
Reference to the mpsTerminalTable, a unique value for each OEM system phone. Range: 1 to 65535
Language
The current display language of the phone device. Enumerations: german (1) dutch (2) english (3) italian (5) danish (6) spanish (7) swedish (8) french (10) portuguese (11) czech (14) norwegian (16) greek (17) icelandic (20) polish (21) hungarian (22) russian (23) romanian (24) slovak (25) turkish (26)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
AutoCallAccept
Defines whether incoming feature calls (e.g. TAPI, announcement, intercom) should be accepted directly: no: no acceptance, normal ringing. via-headset: accept call via a connected headset. via-handsfree: accept call via loudspeaker. Enumerations: no (1) via-headset (2) via-handsfree (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH