>> MIB - Management Information Base
>> Table: mpsDoorIntercomModeTable - (.1.3.6.1.4.1.272.4.53.7.4.1)
Description: This table contains information about door intercom and mode.
mpsDoorIntercomModeTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | Button | DoorButtonIndex | RW
.3 | Number | DoorIntercomModeIndex | RW
.4 | Handling | ENUM | RW
.5 | Assignment | ENUM | RW
.6 | ExtNumber | DisplayString | RW
.7 | AdminStatus | ENUM | D
Index
A unique value for each door intercom. Reference to mpsDoorIntercomIndex. Range: 1 to 10
Button
A unique value for each button of a door intercom. Reference to mpsDoorIntercomSourceButtonIndex. Range: 1 to 4
Number
For each door intercom a variant. Reference to mpsDoorIntercomUserMode. Range: 1 to 10
Handling
Signalling mode (internal) of the door intercom group: simultaneous: all assigned terminals are called simultaneously linear : all assigned terminals are called in the sequence of their entry in configuration. rotating : this call is a special case of the linear call. After all terminals are called, call signalling begins again with the first entered terminal. adding : the terminals are called in the sequence of their entry in the subscriber list. Every terminal that has already been called is called again, until all entered terminals are called. linear-ext : linear + after defined times have run out, all team subscribers can be called in parallel. rotating-ext: rotating + after defined times have run out, all team subscribers can be called in parallel. Enumerations: simultaneous (1) linear (2) rotating (3) adding (4) linear-ext (5) rotating-ext (6)
Assignment
Door intercom group member are internal or one external number. Enumerations: internal (1) external (2)
ExtNumber
This external number will be called, if mpsDoorIntercomModeAssignment = external. Length: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH