>> MIB - Management Information Base
>> Table: bacPropertyStatusTable - (.1.3.6.1.4.1.272.4.60.1.2.1)
Description: One entry in bacPropertyStatusTable.
bacPropertyStatusTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | BwReservedUp | INTEGER | R
.3 | BwReservedDown | INTEGER | R
.4 | BwInterfaceUp | INTEGER | R
.5 | BwInterfaceDown | INTEGER | R
Index
The index in this status table. This index is used to reference the entry in bacPropertyTable where it is used as index as well. Range: 1 to 65535
BwReservedUp
The currently reserved bandwidth for up direction.
BwReservedDown
The currently reserved bandwidth for down direction.
BwInterfaceUp
The bandwidth of the corresponding interface for up direction. 0 if no interface available or no information about interface available.
BwInterfaceDown
The bandwidth of the corresponding interface for down direction. 0 if no interface available or no information about interface available.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH