>> MIB - Management Information Base
>> Table: bacGlobal - (.1.3.6.1.4.1.272.4.60.1.7)
bacGlobal
OID | Name | Type | Access
.1 | AdmissionDefault | ENUM | RW
.2 | DscpSignallingDefault | INTEGER | RW
.3 | DscpAudioDefault | INTEGER | RW
AdmissionDefault
The default behaviour for admission checking, if not any entity relation is configured for a given voip entity. forbidden(1) : Admission is always refused. private-networks-only(2): Admission is granted, if IP of voip entity is a private network address (see RFC 1918 and RFC 5735). unrestriced(3) : Admission is always granted. Enumerations: forbidden (1) private-networks-only (2) unrestriced (3)
DscpSignallingDefault
The 6 bit DSCP value used in IP header for signalling data, if no entry in bacPropertyTable found. Range: 0 to 63
DscpAudioDefault
The 6 bit DSCP value used in IP header for media data, if no entry in bacPropertyTable found. Range: 0 to 63

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH