>> MIB - Management Information Base
>> Table: ttyIfTable - (.1.3.6.1.4.1.272.4.41.1.1)
Description: TTY Port Description Interface entry
ttyIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Name | DisplayString | R
.3 | Network | DisplayString | R
.4 | Profile | ENUM | RW
.5 | Speed | ENUM | RW
.6 | CSQ | INTEGER | R
.7 | AdminStatus | ENUM | RW
.8 | OperStatus | ENUM | R
.9 | Command | DisplayString | R
.10 | Answer | DisplayString | R
.11 | Mode | ENUM | RW
.12 | CurrentMode | ENUM | R
.13 | CurrentSpeed | INTEGER | R
Index
Unique index of the tty Interface.
Name
Name for the Port Length: 0 to 16
Network
GSM Network is actually used Length: 0 to 60
Profile
The profile for this port Enumerations: profile1 (1) profile2 (2) profile3 (3) profile4 (4) profile5 (5)
Speed
The external speed to the modem Enumerations: e9600 (1) e19200 (2) e38400 (3) e57600 (4) e115200 (5) default (6)
CSQ
The GSM receive signal level
AdminStatus
Disable or enbale tty for Modem connection Enumerations: disable (1) enable (2)
OperStatus
Operation state for this port Enumerations: up (1) down (2) init (3) called (4) calling (5) connect (6) simwait (7) pinwait (8) pinerror (9) error (10) disconnected (11)
Command
Last Command to the Modem Length: 0 to 40
Answer
Last Answer from the Modem Length: 0 to 60
Mode
The mode in which the tty interface should operate from now on. Enumerations: disabled (1) aux (2) soip (3) gps (4)
CurrentMode
The current mode in which the tty interface operates now. Enumerations: disabled (1) aux (2) soip (3) gps (4)
CurrentSpeed
The current speed of the tty interface.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH