>> MIB - Management Information Base
>> Table: ipDhcpOptionTable - (.1.3.6.1.4.1.272.4.5.52.6.1)
Description: Arbitrary DHCP options used for DHCP server and BOOTP relay.
ipDhcpOptionTable
OID | Name | Type | Access
.8 | Index | INTEGER | RW
.16 | Enabled | ENUM | D
.24 | GroupID | INTEGER | RW
.32 | GroupDescr | DisplayString | RW
.40 | Code | INTEGER | RW
.48 | ContentType | ENUM | RW
.56 | ContentString | DisplayString | RW
.64 | ContentHex | OCTET STRING | RW
.72 | ContentGroupID | INTEGER | RW
Index
Index of entry. Range: 0 to 65535
Enabled
Enable, disable or delete the table entry. Enumerations: delete (1) true (2) false (3)
GroupID
This object specifies the ID for a group of DHCP options or suboptions. When a DHCP operation refers to such an ID, all options (or suboptions) sharing the same group ID will be added consecutively. Range: 1 to 65535
GroupDescr
A user-friendly name for the group of DHCP options this entry belongs to. Length: 0 to 255
Code
DHCP option code. Range: 0 to 255
ContentType
Content type for this DHCP option. - if set to 'string', the variable part of the DHCP option is filled with the string specified in ipDhcpOptionContentString. - if set to 'hex', the variable part of the DHCP option is filled with the hex content specified in ipDhcpOptionContentHex. - if set to 'group', the variable part of the DHCP option is filled with the collection of DHCP suboptions which share the ipDhcpOptionGroupID value specified in ipDhcpOptionContentGroupID. Enumerations: string (1) hex (2) group (3)
ContentString
This object specifies the content of the string which is used to fill the variable part of the DHCP option when ipDhcpOptionContentType is set to 'string'. Length: 0 to 255
ContentHex
This object specifies the content of the hex buffer which is used to fill the variable part of the DHCP option when ipDhcpOptionContentType is set to 'hex'.
ContentGroupID
This object specifies the ipDhcpOptionGroupID of the group of DHCP suboptions which is used to fill the variable part of the DHCP option when ipDhcpOptionContentType is set to 'group'. If the value is 0, this group has no subelements. Range: 0 to 65535

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH