>> MIB - Management Information Base
>> Table: bridgeTable - (.1.3.6.1.4.1.272.4.56.4.1)
Description: The system will create an entry for each configured bridge. Each entry provides settings for these bridges.
bridgeTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Vlan | ENUM | RW
.3 | WlanFilter | ENUM | RW
Index
Index of the bridge.
Vlan
VLAN operation mode of the bridge: enabled: bridge is VLAN aware disabled: transparent bridge. Enumerations: enabled (1) disabled (2)
WlanFilter
If enabled bridge will drop packets from WLAN ports directed to WLAN ports. Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH