>> MIB - Management Information Base
>> Table: biboAdmCardTable - (.1.3.6.1.4.1.272.4.1.42.1)
Description: The biboAdmCardTable lists installed cards.
biboAdmCardTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Type | DisplayString | R
.3 | State | ENUM | R
.4 | CpldVersion | DisplayString | R
.5 | FpgaVersion | DisplayString | R
.6 | Temp | INTEGER | R
.7 | TempAlarmThreshold | INTEGER | RW
.8 | TempAlarmTrap | ENUM | R
.9 | Admin | ENUM | RW
.10 | TempAlarmThresholdCriticalLow | INTEGER | RW
Slot
The slot, or location of this card. Range: 0 to 31
Type
The name of this card. Length: 0 to 255
State
State of the card. Enumerations: down (1) running (2) fail (3) stopped (4) stopping (5) starting (6)
CpldVersion
Version of onboard CPLD. Length: 0 to 255
FpgaVersion
Version of loaded FPGA firmware. Length: 0 to 255
Temp
This variable shows the actual card temperature in the unit Celsius. Range: 0 to 250
TempAlarmThreshold
Card temperature threshold. Range: 0 to 250
TempAlarmTrap
If the card temperature raises above the threshold, a trap is generated every 60 seconds. Enumerations: normal (1) critical (2)
Admin
Administrative manipulation of card state. Enumerations: up (1) down (2) reconfig (3)
TempAlarmThresholdCriticalLow
Lower Card temperature threshold to return state from critical to normal. Mustn't exceed biboACrdTempAlarmThreshold! When temperature reaches biboACrdTempAlarmThreshold state changes to critical. This state persists until temperature falls below biboACrdTempAlarmThreshUncriticalLow where state changes back to normal. Range: 0 to 250

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH