>> MIB - Management Information Base
>> Table: ip6NetToMediaTable - (.1.3.6.1.4.1.272.4.5.100.2.7.1)
Description: Each entry contains one IPv6 address to `physical' address equivalence.
ip6NetToMediaTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RC
.2 | NetAddress | InetAddressIPv6 | R
.3 | PhysAddress | PhysAddress | R
.4 | Type | ENUM | R
.5 | State | ENUM | R
.6 | LastUpdated | TimeStamp | R
IfIndex
A unique non-zero value identifying the particular IPv6 interface. Range: 1 to 2147483647
NetAddress
The IPv6 Address corresponding to the media-dependent `physical' address. Length: 16 to 16
PhysAddress
The media-dependent `physical' address.
Type
The type of the mapping. The 'dynamic(2)' type indicates that the IPv6 address to physical addresses mapping has been dynamically resolved using the IPv6 Neighbor Discovery protocol. The static(3)' types indicates that the mapping has been statically configured. The local(4) indicates that the mapping is provided for an entity's own interface address. Enumerations: dynamic (1) static (2) local (3)
State
The Neighbor Unreachability Detection [8] state for the interface when the address mapping in this entry is used. Enumerations: incomplete (1) reachable (2) stale (3) delay (4) probe (5) invalid (6) unknown (7)
LastUpdated
The value of sysUpTime at the time this entry was last updated. If this entry was updated prior to the last re-initialization of the local network management subsystem, then this object contains a zero value.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH