>> MIB - Management Information Base
>> Table: potsIfTable - (.1.3.6.1.4.1.272.4.14.1.1.1)
Description: The potsIfTable contains configuration information for the POTS outlets.
potsIfTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | Type | ENUM | RW
.4 | IfMode | ENUM | R
.5 | IfAdminState | ENUM | RW
.6 | IfOperState | ENUM | R
.7 | IfIndex | PotsIfIndex | R
.8 | IfTtxLevel | INTEGER | RW
.9 | IfTtxFreq | ENUM | RW
.10 | IfCoeffIndex | INTEGER | RW
.11 | IfTxGain | INTEGER | RW
.12 | IfRxGain | INTEGER | RW
.13 | IfDialInTimeout | INTEGER | RW
Slot
Identification number of the used slot. Range: 0 to 31
Unit
Identification number of the used unit. Range: 0 to 31
Type
The type of the connected device on socket a. Possible values are: - any(1), (multifunctional) - fax(2), - telephony(3), - modem(4), - disable(5), - doorintercom(6), - answering(7), (-machine) - emergency(8) (-telephone) - alarmInput(9) (sensor function) Enumerations: any (1) fax (2) telephony (3) modem (4) disable (5) doorintercom (6) answering (7) emergency (8) alarmInput (9)
IfMode
Type of outlet. Enumerations: fxo (1) fxs (2)
IfAdminState
This variable allows for taking an POTS interface out of/in service w/o having to touch the configuration. Besides, it is possible to initiate a reconfiguration for that interface in case a mismatch in configuration parameters (hardware vs. software) was detected. Inconsistencies with the need of reconfiguration is a differing potsIfMode (fxo/fxs). In case of mismatch, contents of this variable might be wrong and this circumstance is reflected in variable potsIfOperState. State reconfig may then be used in order to cause an update of these variable as appropriate which ... - will be signalled to higher protocol layers, and - can result in extensive reconfiguration steps The latter may also cover clean-ups undoable by system so this decision is left to the user. Default value is down. Enumerations: down (1) up (2) reconfig (3)
IfOperState
The operational state of an interface is indicated via this variable. Possible values are: - down(1), - running(2), - fail(3), - not-connected(4), - stopped(5), - stopping(6), - starting(7), The latter two states being of transitional type, mainly for hot-plug type hardware, and won't be normally seen by user. State fail is used to reflect inconsistencies between hardware state and configuration concerning interface mode (potsIfMode). Enumerations: down (1) running (2) fail (3) not-connected (4) stopped (5) stopping (6) starting (7)
IfIndex
Reference to the FXS or FXO table.
IfTtxLevel
Teletax (metering pulse) level: for FXS lines: output level for FXO lines: minimum level Range: -50 to 0
IfTtxFreq
Teletax (metering pulse) frequency: 1: no teletax output/reception 3: 12 kHz 4: 16 kHz Enumerations: off (1) freq12khz (3) freq16khz (4)
IfCoeffIndex
Selection of the coefficient set provided by the FXS or FXO line driver. This allows to use specific settings with e.g. resistive or complex line impedances. Supported values are: 600: 600 ohms (resistive) 1155: german Zr (complex) 1170: ETSI (complex)
IfTxGain
Amplification or attenuation (negative gain) of outgoing audio in dB. Range: -30 to 10
IfRxGain
Amplification or attenuation (negative gain) of incoming audio in dB. Range: -30 to 10
IfDialInTimeout
Limit for time interval between two consecutive dialling digits. Range: 1 to 99

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH