>> MIB - Management Information Base
>> Table: ipsecPeerTrafficTable - (.1.3.6.1.4.1.272.4.26.29.1)
Description: This table contains peer related lists of traffic permitted for Phase 2 negotiation. Note that this table contains optional entries solely, in the default case (no entries) subsequently no restriction will take place.
ipsecPeerTrafficTable
OID | Name | Type | Access
.1 | Ifindex | INTEGER | RW
.2 | Description | DisplayString | RW
.3 | LocalAddress | IpAddress | RW
.4 | LocalMask | IpAddress | RW
.5 | LocalPort | INTEGER | RW
.6 | LocalPortRange | INTEGER | RW
.7 | RemoteAddress | IpAddress | RW
.8 | RemoteMask | IpAddress | RW
.9 | RemotePort | INTEGER | RW
.10 | RemotePortRange | INTEGER | RW
.11 | Protocol | ENUM | RW
.12 | Policy | ENUM | D
.13 | Type | ENUM | RW
.14 | Ip6LocalAddress | InetAddressIPv6 | RW
.15 | Ip6LocalMaskLen | INTEGER | RW
.16 | Ip6RemoteAddress | InetAddressIPv6 | RW
.17 | Ip6RemoteMaskLen | INTEGER | RW
.18 | ChildXrt | INTEGER | R
Ifindex
.
Description
An optional human readable description for this entry.
LocalAddress
The local IPv4-address of this entry. It maybe either a single address or a network address (in combination with ipsecPeerTrafficLocalMask).
LocalMask
The length of the network mask for a local network.
LocalPort
The local port defined for this entry.
LocalPortRange
The local port range defined for this entry.
RemoteAddress
The remote IPv4-address of this entry. It maybe either a single address or a network address (in combination with ipsecPeerTrafficRemoteMask).
RemoteMask
The network mask for a remote network.
RemotePort
The remote UDP/TCP port defined for this entry.
RemotePortRange
The remote UDP/TCP port range defined for this entry.
Protocol
The transport protocol defined for this entry.
Policy
This object specifies whether this network policy is used for inbound, outbound or both processing. Possible values: delete(1) -- delete this entry role-initiator(2) -- P2 initiator mode traffic policy role-responder(3) -- P2 responder mode traffic policy both(4) -- P2 initiator as well as responder traffic policy role-initiator-syncrt(5) -- P2 initiator mode + ipExtRt filter both-syncrt(6) -- P2 initiator/responder + ipExtRt filter.
Type
Defines the site of selection criteria for packets that are contained in this entry. local -- local selection criteria remote -- remote selection cribteria both-sides -- local and remote selection criteria
Ip6LocalAddress
The local IPv6 address of this entry. It maybe either a staring address (in combination with ipsecPeerTrafficIp6LocalRange) or a network address (in combination with ipsecPeerTrafficIp6LocalMaskLen). (for IKEv2 only)
Ip6LocalMaskLen
Indicates the prefix length associated with the local IPv6 address (in combination with ipsecPeerTrafficIp6LocalAddress). (for IKEv2 only)
Ip6RemoteAddress
The remote IPv6 address of this entry. It maybe either a starting address (in combination with ipsecPeerTrafficIp6RemoteRange) or a network address (in combination with ipsecPeerTrafficRemoteMaskLen). (for IKEv2 only)
Ip6RemoteMaskLen
Indicates the prefix length associated with the remote IPv6 address (in combination with ipsecPeerTrafficIp6RemoteAddress). (for IKEv2 only)
ChildXrt
Row number of the associated ipExtRtTable entry.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH