>> MIB - Management Information Base
>> Table: sysStat - (.1.3.6.1.4.1.272.4.17.500)
sysStat
OID | Name | Type | Access
.1 | BootConfig | ENUM | R
.2 | FunctionState | ENUM | R
.3 | OperationMode | ENUM | R
.4 | ConfigConvert | ENUM | RW
.5 | ConfigConvertState | ENUM | R
BootConfig
After system boot this variable shows which configuration was loaded: none: no configuration whatsoever bootfac: factory boot configuration default: default configuration as provided by image boot: configuration found in flash. Enumerations: none (1) bootfac (2) default (3) boot (4)
FunctionState
This variable contains the current function state, which is toggeled by pressing the function button on the device. Enumerations: on (1) off (2)
OperationMode
This variable defines the operation mode of the device concerning telephony functionality. If any voice functionality is integrated it can be either mgw(1) for Media GateWay functionality of pbx(2) for a full-fledged telephone system. For systems w/o voice functionality the variable has value plain(0). Enumerations: plain (0) mgw (1) pbx (2)
ConfigConvert
This variable triggers the conversion of configuration between pbx and mediagateway. Setting the variable to start indicates the beginning of conversion. The variable is reset to idle immediately. A conversion is only possible once during system uptime. Enumerations: idle (1) start (2)
ConfigConvertState
This variable shows the state of the converter idle - no conversion performed since uptime progress - conversion in progress done - conversion successfully completed failed - conversion erroneously ended The value progress is shown during the conversion. The values done and failed are final states and indicate the completion of conversion. Enumerations: idle (1) progress (2) done (3) failed (4)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH