>> MIB - Management Information Base
>> Table: ip6AdmPrefixTable - (.1.3.6.1.4.1.272.4.5.100.1.4.1)
Description: An interface entry containing objects of a particular IPv6 address prefix.
ip6AdmPrefixTable
OID | Name | Type | Access
.1 | Id | Unsigned32 | RC
.2 | IfIndex | InterfaceIndexOrZero | RC
.3 | AdminStatus | ENUM | D
.4 | Type | ENUM | RC
.5 | Prefix | InetAddressIPv6 | RC
.6 | Length | INTEGER | RC
.7 | NextHop | InetAddressIPv6 | RC
.8 | Slaac | ENUM | RC
.9 | Descr | DisplayString | RC
Id
A unique non-zero value identifying the particular IPv6 prefix.
IfIndex
A unique non-zero value identifying the particular IPv6 interface or relay. Range: 0 to 2147483647
AdminStatus
The administrative status of this entry. Enumerations: enable (1) disable (2) delete (3)
Type
The type of the prefix associated with the this interface. Enumerations: dynamic (1) static (2)
Prefix
The prefix associated with the this interface. Length: 16 to 16
Length
The length of the prefix (in bits). Range: 0 to 128
NextHop
The next hop associated with this prefix. Length: 16 to 16
Slaac
SLAAC method, this setting determines the address format which should be the result of the address autoconfiguration procedure eui64 EUI-64-Identifier according RFC 4291 privacy-ext Privacy Extensions according RFC 4941 disabled no SLAAC Enumerations: eui64 (1) disabled (3)
Descr
User defined description of this prefix entry Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH