>> MIB - Management Information Base
>> Table: trempPersist - (.1.3.6.1.4.1.272.4.99.1.2)
trempPersist
OID | Name | Type | Access
.1 | MonitoringInterval | INTEGER | R
.2 | CertIndex | INTEGER | R
.3 | HMAC | OCTET STRING | R
.4 | HMACTimestamp | INTEGER | R
MonitoringInterval
The interval in seconds to send to the TREMP server the monitoring events. Range: 5 to 3600
CertIndex
Index of certificate entry in certTable which is to be used as client certificate for REST transport.
HMAC
Current HMAC key for non 'https' connections. Length: 20 to 20
HMACTimestamp
Timestamp that define the HMAC valid lifetime

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH