>> MIB - Management Information Base
>> Table: ip6DynRouteTable - (.1.3.6.1.4.1.272.4.5.100.2.9.1)
Description: A dynamically created routing entry.
ip6DynRouteTable
OID | Name | Type | Access
.1 | Creator | ENUM | R
.2 | Target | InetAddressIPv6 | R
.3 | TargetLen | INTEGER | R
.4 | Source | InetAddressIPv6 | R
.5 | SourceLen | INTEGER | R
.6 | IfIndex | InterfaceIndex | R
.7 | NextHop | InetAddressIPv6 | R
.8 | Priority | INTEGER | R
Creator
The creator of the dynamic routing-entry, can be DHCPv6 or any other (routing-)protocol. Enumerations: netmgmt (2) rip (4) ospf (5) bgp (6) idrp (7) dhcp-pd (8)
Target
The destination IPv6 address of this route. This object may not take a multicast address value. Length: 16 to 16
TargetLen
Indicates the prefix length of the destination address. Range: 0 to 128
Source
The Source IPv6 address of this route. This object may not take a multicast address value. Length: 16 to 16
SourceLen
Indicates the prefix length of the source address. Range: 0 to 128
IfIndex
The index value which uniquely identifies the local interface through which the next hop of this route should be reached. The interface identified by a particular value of this index is the same interface as identified by the same value of ip6DeviceIfIndex. For routes of the discard type this value can be zero. Range: 1 to 2147483647
NextHop
On remote routes, the address of the next hop of this routing entry, set to :: otherwise. Length: 16 to 16
Priority
The routing priority for this route, a value of 0 means highest priority, a value of 16 lowest priority. Range: 0 to 16

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH