>> MIB - Management Information Base
>> Table: systemPhoneFeatureControlTable - (.1.3.6.1.4.1.272.4.64.7.1.1)
Description: This table contains status information about each PBX feature key subscribed by Gigaset System Phones.
systemPhoneFeatureControlTable
OID | Name | Type | Access
.1 | Index | SystelFeatureCtrlIndex | R
.2 | FKType | ENUM | R
.3 | Count | INTEGER | R
.4 | Status | ENUM | R
.5 | ExtIndex | INTEGER | R
.6 | Code | DisplayString | R
.7 | Silent | ENUM | RW
.8 | AdminStatus | ENUM | D
Index
A unique index referenced by the systemPhoneFeatureLinkTable. Range: 1 to 65535
FKType
Type of the PBX feature key, see description of 'systemPhoneFKType'. Enumerations: dial-standard (1) dial-dtmf (2) dial-keypad (3) extension-subscriber (4) extension-team (5) trunk-line (6) team-log (7) system-call-announce (8) system-call-announce-allow (9) system-call-exchange (10) system-call-exchange-allow (11) boss-boss (12) boss-secretary (13) boss-diversion (14) call-forwarding-cfu (15) call-forwarding-cfb (16) call-forwarding-cfnr (17) macro (18) headset (19) auto-accept (20) bundle (21) connection (22) system-parking (23) internal-line-access (24) hotel-room (25) agent-time (26) night-mode (27) hotel-room-connect (28) agent-time-renew (29) do-not-disturb (30) shift (31) parallel-ringing (32) nop (33) system-call-announce-team (34) msn-selection (35) xml-content (50) next-call-anonymous (51) menu-call-divert (52) menu-resource-dir (53) menu-internet-radio (54) toggle-call-divert (55) not-configured (99)
Count
Counts the number of systemPhoneFunctionKeyEntry's referencing this table. Only used if a non MSN related feature must be controlled e.g. PBX night-mode.
Status
The current LED status for the PBX feature key. Enumerations: led-off (0) led-on (1) led-blink (2)
ExtIndex
A reference to the mpsExtensionTable. Set to 0 if a non MSN related feature must be controlled e.g. PBX night-mode. Range: 0 to 65535
Code
The Gigaset 'Service Code' provisioning parameter. This code is generated via a special coding algorithm by the PBX system. Length: 0 to 32
Silent
Defines whether the phone loudspeaker should be turned off or on automatically during the PBX feature call is established. Enumerations: true (1) false (2)
AdminStatus
Just for MIB entry deletion. Enumerations: enabled (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH