>> MIB - Management Information Base
>> Table: biboPPPIpPoolTable - (.1.3.6.1.4.1.272.4.3.17.1)
Description: Pool of IP addresses for dynamic IP address assignment via IPCP. See the biboPPPIpAddress field for further explanation.
biboPPPIpPoolTable
OID | Name | Type | Access
.1 | Identifier | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Mode | ENUM | RW
Identifier
The ID of the responding dynamic pool.
AdminStatus
If the AdminStatus is set to enabled(1) this entry will be used. Setting it to disabled(2) this entry won't be used . You may also delete this entry by changing it to delete(3). Enumerations: enabled (1) disabled (2) delete (3)
Mode
The IpPoolMode tries to reassign the IP Address a client had before if it is in recover(1) Mode. Otherwise (2) an unassigned IP Address of the PPP dynamic IP Pool is assigned to the client no matter which Address he had before. Enumerations: recover (1) random (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH