>> MIB - Management Information Base
>> Table: pimNeighborTable - (.1.3.6.1.4.1.272.4.5.54.2.1.2.1)
Description: An entry (conceptual row) in the pimNeighborTable.
pimNeighborTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | AddressType | ENUM | R
.3 | Address | InetAddressIPv6 | R
.4 | UpTime | TimeTicks | R
.5 | ExpiryTime | TimeTicks | R
.6 | LanPruneDelayPresent | ENUM | R
.7 | PropagationDelay | Unsigned32 | R
.8 | OverrideInterval | Unsigned32 | R
.9 | TBit | ENUM | R
.10 | GenerationIDPresent | ENUM | R
.11 | GenerationIDValue | Unsigned32 | R
.12 | BidirCapable | ENUM | R
.13 | DRPriorityPresent | ENUM | R
.14 | DRPriority | Unsigned32 | R
.15 | SRCapable | ENUM | R
IfIndex
The value of ifIndex for the interface used to reach this PIM neighbor. Range: 1 to 2147483647
AddressType
The address type of this PIM neighbor. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Address
The primary IP address of this PIM neighbor. The InetAddressType is given by the pimNeighborAddressType object. Length: 16 to 16
UpTime
The time since this PIM neighbor (last) became a neighbor of the local router.
ExpiryTime
The minimum time remaining before this PIM neighbor will be aged out. The value zero indicates that this PIM neighbor will never be aged out.
LanPruneDelayPresent
Evaluates to TRUE if this neighbor is using the LAN Prune Delay option. Enumerations: true (1) false (2)
PropagationDelay
The value of the Propagation_Delay field of the LAN Prune Delay option received from this neighbor. This object is always zero if pimNeighborLanPruneDelayPresent is FALSE. Range: 0 to 32767
OverrideInterval
The value of the Override_Interval field of the LAN Prune Delay option received from this neighbor. This object is always zero if pimNeighborLanPruneDelayPresent is FALSE. Range: 0 to 65535
TBit
Whether the T bit was set in the LAN Prune Delay option received from this neighbor. The T bit specifies the ability of the neighbor to disable join suppression. This object is always TRUE if pimNeighborLanPruneDelayPresent is FALSE. Enumerations: true (1) false (2)
GenerationIDPresent
Evaluates to TRUE if this neighbor is using the Generation ID option. Enumerations: true (1) false (2)
GenerationIDValue
The value of the Generation ID from the last PIM Hello message received from this neighbor. This object is always zero if pimNeighborGenerationIDPresent is FALSE.
BidirCapable
Evaluates to TRUE if this neighbor is using the Bidirectional-PIM Capable option. Enumerations: true (1) false (2)
DRPriorityPresent
Evaluates to TRUE if this neighbor is using the DR Priority option. Enumerations: true (1) false (2)
DRPriority
The value of the Designated Router Priority from the last PIM Hello message received from this neighbor. This object is always zero if pimNeighborDRPriorityPresent is FALSE.
SRCapable
Evaluates to TRUE if this neighbor is using the State Refresh Capable option. This object is used only by PIM-DM. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH