>> MIB - Management Information Base
>> Table: ip6ContextTable - (.1.3.6.1.4.1.272.4.5.100.3.2.1)
Description: Contains a IPv6 Stateful Inspection Firewall (SIF) policy.
ip6ContextTable
OID | Name | Type | Access
.1 | Ident | INTEGER | R
.2 | Protocol | ENUM | R
.3 | InitiatorIfIndex | InterfaceIndexOrZero | R
.4 | InitiatorAddress | InetAddressIPv6 | R
.5 | InitiatorPort | INTEGER | R
.6 | ResponderIfIndex | InterfaceIndexOrZero | R
.7 | ResponderAddress | InetAddressIPv6 | R
.8 | ResponderPort | INTEGER | R
.9 | RouteFlags | BITS | R
.10 | Lifetime | INTEGER | R
.11 | Age | TimeStamp | R
Ident
Internal ID for the context entry.
Protocol
IP protocol associated with this context. Enumerations: icmp (1) igmp (2) ggp (3) ip (4) tcp (6) egp (8) igp (9) pup (12) chaos (16) udp (17) hmp (20) xns-idp (22) rdp (27) ipv6 (41) rsvp (46) gre (47) esp (50) ah (51) tlsp (56) skip (57) icmpv6 (58) kryptolan (65) iso-ip (80) igrp (88) ospf (89) ipip (94) pim (103) ipx-in-ip (111) vrrp (112) l2tp (115)
InitiatorIfIndex
Initiators interface index. Range: 0 to 2147483647
InitiatorAddress
Initiators IPv6 address. Length: 16 to 16
InitiatorPort
Initiators TCP/UDP port number. Range: 0 to 65535
ResponderIfIndex
Responders interface index. Range: 0 to 2147483647
ResponderAddress
Responders IPv6 address. Length: 16 to 16
ResponderPort
Responders TCP/UDP port number. Range: 0 to 65535
RouteFlags
various routing flags: local: Source or target is local direct: Source or target direct routing deny: drop rule or firewall blocked reject: icmp answer by no route or firewall blocked blocked: set by firewall rule deny or reject Enumerations: local (0) direct (1) deny (2) reject (3) blocked (4)
Lifetime
The 'Lifetime' of this context in seconds.
Age
The age of this context in seconds.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH