>> MIB - Management Information Base
>> Table: systemPhoneIPTable - (.1.3.6.1.4.1.272.4.64.1.5.1)
Description: This table contains data assigned to network/ip-configuration of the system phone.
systemPhoneIPTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | Facility | BITS | R
.3 | MacAddress | MacAddress | R
.4 | Address | IpAddress | RW
.5 | GatewayAddress | IpAddress | RW
.6 | RegistrarAddress | IpAddress | RW
.7 | Subnetmask | IpAddress | R
Index
A reference to systemPhoneTable (or mpsTerminalTable). Range: 1 to 65535
Facility
IP facility bit matrix: dhcp: 0, system phone uses a dhcp-server, the ip address of this dhcp-server is stored in systemIPGatewayAddress. 1, system phone don't uses a dhcp-server, the ip address stored in systemPhoneIPGateway is the standard gateway of systemphone. gateway-equals-registrar: 0, system phone gateway address is different to registrar address for sip registration. 1, system phone gateway address equals registrar address for sip registration. Enumerations: dhcp (0) gateway-equals-registrar (1)
MacAddress
Variable contains the MAC-Address of the system phone. Length: 6 to 6
Address
Variable contains the IP-Address of the system phone.
GatewayAddress
Variable contains the IP address of standard gateway.
RegistrarAddress
Variable contains the IP address of registrar server (in system phone the registrar server is mentioned as SysServer).
Subnetmask
Variable contains the subnetmask which the system phone will use for the IP address.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH