>> MIB - Management Information Base
>> Table: soipConfigTable - (.1.3.6.1.4.1.272.4.58.1.1)
Description: The soipConfigEntry contains configuration data of the SoIP module.
soipConfigTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | UartBaud | INTEGER | RW
.3 | UartDataBits | INTEGER | RW
.4 | UartParity | ENUM | RW
.5 | UartStopBits | INTEGER | RW
.6 | UartHandshake | ENUM | RW
.7 | UartSendGraciousXonXoff | ENUM | RW
.8 | IpProtocol | ENUM | D
.9 | IpReconnectTimeout | INTEGER | RW
.10 | IpLocalIp | IpAddress | RW
.11 | IpLocalPort | INTEGER | RW
.12 | IpRemoteIp | IpAddress | RW
.13 | IpRemotePort | INTEGER | RW
.14 | IpIfIndex | INTEGER | RW
.15 | TriggerByteCount | INTEGER | RW
.16 | TriggerDelay | INTEGER | RW
.17 | TriggerTimeout | INTEGER | RW
.18 | BufferClear | ENUM | RW
Index
Reference to the used serial port.
UartBaud
Baud rate of serial port. Range: 1 to 115200
UartDataBits
Data bits of serial port. Range: 7 to 8
UartParity
Type of serial port. none(1) -- No parity bit even(2) -- Even parity bit odd(3) -- Odd parity bit Enumerations: none (1) even (2) odd (3)
UartStopBits
Stop bits of serial port. Range: 1 to 2
UartHandshake
Handshake used on serial port. none(1) -- no handshake rts-cts(2) -- RTS/CTS signal pair used for handshake (hardware) xon-xoff(3) -- XOn/XOff bytes used for handshake (software) Received XOn/XOff characters are not forwarded via IP. Enumerations: none (1) rts-cts (2) xon-xoff (3)
UartSendGraciousXonXoff
Send gracious XOn/XOff. TCP: if IP connection is established/closed UDP: send XOn on startup Enumerations: true (1) false (2)
IpProtocol
IP protocol and mode to use. tcp-server(1) -- Wait for incoming TCP connections tcp-client(2) -- Active connect via TCP udp(3) -- UDP With delete(15) the entry will be deleted Enumerations: tcp-server (1) tcp-client (2) udp (3) delete (15)
IpReconnectTimeout
TCP client: Retry connect after n seconds if connection is refused or not answered. 0 = do not reconnect Range: 0 to 65535
IpLocalIp
TCP server: accept connection only on this IP. 0=any. TCP client: issue connection from this IP. 0=automatic. UDP unicast: send data from and accept on this IP. 0=automatic. UDP multicast master (1:n): master unicast IP. 0=automatic. UDP multicast slave (1:n): multicast group IP. UDP multicast multi-master (n:m): multicast group IP.
IpLocalPort
TCP server: local port to listen on for connections TCP client: local port to issue connection from. 0=automatic. UDP unicast: port to send from / receive on. 0=automatic. UDP multicast: port to send from / receive on. 0=automatic. Range: 0 to 65535
IpRemoteIp
TCP server: accept connection only from this IP. 0=any. TCP client: issue connection to this IP. UDP unicast: send data to this IP. UDP multicast master (1:n): multicast group IP. UDP multicast slave (1:n): master unicast IP. UDP multicast multi-master (n:m): multicast group IP.
IpRemotePort
TCP server: remote port to accept connections from. 0=any. TCP client: remote port to connect to UDP unicast: port to send to / receive from. UDP multicast: port to send to / receive on Range: 0 to 65535
IpIfIndex
Interface index to bind to. TCP server: ignored TCP client: ignored UDP unicast: ignored UDP multicast: multicast interface index
TriggerByteCount
Send an IP packet after receiving n bytes from serial port. Range: 1 to 1460
TriggerDelay
Send an IP packet n milliseconds after receiving the first byte from serial port. 0 = trigger disabled Range: 0 to 65535
TriggerTimeout
Send an IP packet n milliseconds after receiving the last byte from serial port. 0 = trigger disabled Range: 0 to 65535
BufferClear
Trigger clearing of buffers. Variable falls back to no-action after clearing the buffers. no-action(1) -- clear nothing, normal operation serial-rx(2) -- clear serial Rx buffer serial-tx(3) -- clear serial Tx buffer serial-rx-tx(4) -- clear serial Rx and Tx buffer Enumerations: no-action (1) serial-rx (2) serial-tx (3) serial-rx-tx (4)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH