>> MIB - Management Information Base
>> Table: igmpSrcListTable - (.1.3.6.1.4.1.272.4.5.51.4.1)
Description: An entry (conceptual row) in the igmpSrcListTable.
igmpSrcListTable
OID | Name | Type | Access
.1 | Address | IpAddress | R
.2 | IfIndex | InterfaceIndex | R
.3 | HostAddress | IpAddress | R
.4 | Status | ENUM | D
.5 | Timer | TimeTicks | R
.6 | Self | ENUM | R
Address
The igmpCacheAddress value (multicast-group-address) of the related igmpCacheTable entry.
IfIndex
The igmpCacheIfIndex value (interface-index) of the related igmpCacheTable entry. Range: 1 to 2147483647
HostAddress
The source-address (multicast-sender) specified by this entry. The igmpCacheSourceFilterMode value (filter-mode) of the related igmpCacheTable entry tells if this source is included or excluded.
Status
The status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)
Timer
The time when this entry will be aged out.
Self
Tells if the local system is a member of this entity. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH