>> MIB - Management Information Base
>> Table: wlcWTPTable - (.1.3.6.1.4.1.272.4.61.1.3.1)
Description: The wlcWTPTable contains information relating to the WTPs currently managed by our Access Controller (AC). Each entry corresponds to a managed Wireless Termination Point (WTP). Entries can be added or deleted by the user.
wlcWTPTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | OperStatus | ENUM | R
.4 | MacAddress | MacAddress | RW
.5 | Description | DisplayString | RW
.6 | Name | DisplayString | RW
.7 | Location | DisplayString | RW
.8 | AdminSwVer | DisplayString | RW
.9 | Encryption | ENUM | RW
.10 | TriggerStat | ENUM | RW
.11 | secIndex | INTEGER | RW
.12 | authEapolIndex | INTEGER | RW
.13 | globalIndex | INTEGER | RW
.14 | radiusSrvIndex | INTEGER | RW
.15 | logHostIndex | INTEGER | RW
.17 | localServicesIndex | INTEGER | RW
.23 | presenceProfIndex | INTEGER | RW
Index
Unique index for the WTP.
AdminStatus
Enable, disable or delete the requested WTP. Enumerations: disabled (1) enabled (2) delete (32)
OperStatus
This notification shows if the WTP is currently operative. Enumerations: disabled (1) enabled (2) initialising (3) no-license-available (4)
MacAddress
First ethernet MAC address of the WTP. Length: 6 to 6
Description
Description of the requested WTP. Length: 0 to 63
Name
Name of the requested WTP. Length: 0 to 63
Location
Location of the requested WTP. Length: 0 to 63
AdminSwVer
This variable displays the current software version of each WTP Length: 0 to 31
Encryption
Enable or disable the encryption between AC and WTP. Enumerations: enabled (1) disabled (2)
TriggerStat
Setting this variable to update(2) the WTP is triggered to send statistics (VSS, ACLDenied, stations, ...). After the trigger is sent it is switched back to idle(1). Default is idle(1). Enumerations: idle (1) update (2)
secIndex
This attribute shows the currently configured secIndex of the requested WTP.
authEapolIndex
This attribute shows the currently configured EapolIndex of the requested WTP.
globalIndex
This attribute shows the currently configured globalIndex of the requested WTP.
radiusSrvIndex
This attribute shows the currently configured radiusSrvIndex of the requested WTP.
logHostIndex
This attribute shows the currently configured logHostIndex of the requested WTP.
localServicesIndex
This attribute shows the currently configured localServicesIndex of the requested WTP.
presenceProfIndex
Sets the Presence Analytics profile for this WTP.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH