>> MIB - Management Information Base
>> Table: mpsCallTransactionTable - (.1.3.6.1.4.1.272.4.53.17.1.1)
Description: This table contains status information about each transaction.
mpsCallTransactionTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | R
.2 | Type | ENUM | R
.3 | LocalNumber | DisplayString | R
.4 | RemoteNumber | DisplayString | R
.5 | RedirectNumber | DisplayString | R
.6 | Direction | ENUM | R
.7 | State | ENUM | R
.8 | Channel | Unsigned32 | R
.9 | IfIndex | InterfaceIndex | R
Index
A unique ID for each transaction.
Type
This variable contains the transaction type: subscriber: transaction to/from internal subscriber. trunk: transaction to/from trunk port. parking: a parked call due to open-inquiry request Enumerations: subscriber (1) trunk (2) parking (3)
LocalNumber
This variable contains the local number of the transaction: for mpsCallTransType = subscriber: the number of the internal extension for mpsCallTransType = trunk : the MSN or DDI of the trunk port. for mpsCallTransType = parking : the system call number of the respective parking place Length: 0 to 32
RemoteNumber
This variable contains the remote number of the transaction: for mpsCallTransType = subscriber: the MSN or DDI of the trunk port for mpsCallTransType = trunk : the calling party (for incoming calls) or the called party (for outgoing calls). Length: 0 to 32
RedirectNumber
This variable contains the redirected or redirection number for redirected transactions. Length: 0 to 32
Direction
description not available Enumerations: initiator (1) recipient (2)
State
This variable contains the state of the transaction. Enumerations: idle (1) alert (2) connect (3) held (4) release (5)
Channel
The corresponding channel number for this transaction.
IfIndex
The corresponding interface used for this transaction. Range: 1 to 2147483647

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH