>> MIB - Management Information Base
>> Table: qosPolicyStatTable - (.1.3.6.1.4.1.272.4.27.4.1)
Description: The qosPolicyStatTable contains statistical QoS-specific information for the policy specified by qosPolicyStatIfIndex (interface index), qosPolicyStatType and qosPolicyStatClassId. Only the system can add or delete entries to this table.
qosPolicyStatTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Type | ENUM | R
.3 | ClassId | INTEGER | R
.4 | OutPkts | Counter32 | R
.8 | PktsQueued | Counter32 | R
.9 | OctetsQueued | Counter32 | R
.10 | PktsDropped | Counter32 | R
.15 | State | ENUM | RW
.16 | Throughput | INTEGER | R
.17 | HCOutOctets | Counter64 | R
.18 | HCOctetsDropped | Counter64 | R
.19 | RttRate | INTEGER | R
.20 | Descr | DisplayString | R
IfIndex
The unique interface index
Type
The related type of packet classes for this QoS policy (see qosPolicyType for further explanation). Enumerations: class-based (1) high-priority (2) default (3)
ClassId
Unique packet class ID
OutPkts
The number of packets sent belonging to the related packet class.
PktsQueued
The number of data packets of the related class enqueued and waiting to be sent.
OctetsQueued
The representation of qosPolicyStatPktsQueued in octets.
PktsDropped
The number of data packets of the related class dropped during congestion.
State
This object allows statistics to be reinitialized. Possible values: running(1) = no reset of statistics reset(2) = reset all counters in this entry except counters for queued packets and octets. When the reset action is over, this object is automatically restored to its 'running(1)' default state. Enumerations: running (1) reset (2)
Throughput
The actual amout of bits transmitted per second.
HCOutOctets
The representation of qosPolicyStatOutPkts in octets.
HCOctetsDropped
The representation of qosPolicyStatPktsDropped in octets
RttRate
The current RTT traffic rate (in bits per second) for this queue in case of activated real-time mode.
Descr
A textual string describing this QoS policy, copied from associated qosPolicyTable entry. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH