>> MIB - Management Information Base
>> Table: wlanVSSBadAuthAcctTable - (.1.3.6.1.4.1.272.4.46.28.1)
Description: The wlanVSSBadAuthAcct containes some authentication accounting parameters for a VSS.
wlanVSSBadAuthAcctTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | STAMac | MacAddress | R
.3 | Time1stFail | Date | R
.4 | TimeLastFail | Date | R
.5 | NumFailAttempts | INTEGER | R
.6 | LastRSSI | INTEGER | R
Index
Reference to VSS Entry this authentication accounting information corresponds to.
STAMac
The MAC address of the station the failed authentication attempts are originating from.
Time1stFail
Timestamp of the first failed authentication attempt. This entry is deleted after 1 hour of inactivity.
TimeLastFail
Timestamp of the last failed authentication attempt.
NumFailAttempts
The number of failed authentication attempts from a given station on a given VSS since the first failed authentication attempt within an hour.
LastRSSI
The last RSSI the station had.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH