>> MIB - Management Information Base
>> Table: mpsDeviceVirtualTable - (.1.3.6.1.4.1.272.4.53.3.2.1)
Description: This table contains information for each virtual device.
mpsDeviceVirtualTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Mode | ENUM | RW
.3 | DefaultExtension | ExtensionIndexOrZero | RW
.4 | AdminStatus | ENUM | D
Index
A unique value for each virtual device.
Mode
Contains mode of the device. Enumerations: capi (1) ipline-pmp (2) router (3) iptrunk (4)
DefaultExtension
Contains the extension index of an internal device port, for default. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2) disable (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH