>> MIB - Management Information Base
>> Table: wlanBridgeLinkHTStatsTable - (.1.3.6.1.4.1.272.4.46.34.1)
Description: The wlanBridgeLinkHTStatsTable contains additional statistical data about 802.11n HT frames related to WLAN bridge links (WBL).
wlanBridgeLinkHTStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Address | MacAddress | R
.3 | RxFramesMCS0 | Counter32 | R
.4 | RxFramesMCS1 | Counter32 | R
.5 | RxFramesMCS2 | Counter32 | R
.6 | RxFramesMCS3 | Counter32 | R
.7 | RxFramesMCS4 | Counter32 | R
.8 | RxFramesMCS5 | Counter32 | R
.9 | RxFramesMCS6 | Counter32 | R
.10 | RxFramesMCS7 | Counter32 | R
.11 | RxFramesMCS8 | Counter32 | R
.12 | RxFramesMCS9 | Counter32 | R
.13 | RxFramesMCS10 | Counter32 | R
.14 | RxFramesMCS11 | Counter32 | R
.15 | RxFramesMCS12 | Counter32 | R
.16 | RxFramesMCS13 | Counter32 | R
.17 | RxFramesMCS14 | Counter32 | R
.18 | RxFramesMCS15 | Counter32 | R
.19 | RxFramesMCS16 | Counter32 | R
.20 | RxFramesMCS17 | Counter32 | R
.21 | RxFramesMCS18 | Counter32 | R
.22 | RxFramesMCS19 | Counter32 | R
.23 | RxFramesMCS20 | Counter32 | R
.24 | RxFramesMCS21 | Counter32 | R
.25 | RxFramesMCS22 | Counter32 | R
.26 | RxFramesMCS23 | Counter32 | R
.27 | TxFramesMCS0 | Counter32 | R
.28 | TxFramesMCS1 | Counter32 | R
.29 | TxFramesMCS2 | Counter32 | R
.30 | TxFramesMCS3 | Counter32 | R
.31 | TxFramesMCS4 | Counter32 | R
.32 | TxFramesMCS5 | Counter32 | R
.33 | TxFramesMCS6 | Counter32 | R
.34 | TxFramesMCS7 | Counter32 | R
.35 | TxFramesMCS8 | Counter32 | R
.36 | TxFramesMCS9 | Counter32 | R
.37 | TxFramesMCS10 | Counter32 | R
.38 | TxFramesMCS11 | Counter32 | R
.39 | TxFramesMCS12 | Counter32 | R
.40 | TxFramesMCS13 | Counter32 | R
.41 | TxFramesMCS14 | Counter32 | R
.42 | TxFramesMCS15 | Counter32 | R
.43 | TxFramesMCS16 | Counter32 | R
.44 | TxFramesMCS17 | Counter32 | R
.45 | TxFramesMCS18 | Counter32 | R
.46 | TxFramesMCS19 | Counter32 | R
.47 | TxFramesMCS20 | Counter32 | R
.48 | TxFramesMCS21 | Counter32 | R
.49 | TxFramesMCS22 | Counter32 | R
.50 | TxFramesMCS23 | Counter32 | R
.51 | RxBandwidth | ENUM | R
.52 | RxGuardInterval | ENUM | R
.53 | TxBandwidth | ENUM | R
.54 | TxGuardInterval | ENUM | R
IfIndex
System generated unique WLAN bridge link index.
Address
Address where the WBL slave is associated with. Or on WBL master it is the MAC-Address of the connected WBL slave.
RxFramesMCS0
This attribute shows the number of HT data frames that were received at MCS 0.
RxFramesMCS1
This attribute shows the number of HT data frames that were received at MCS 1.
RxFramesMCS2
This attribute shows the number of HT data frames that were received at MCS 2.
RxFramesMCS3
This attribute shows the number of HT data frames that were received at MCS 3.
RxFramesMCS4
This attribute shows the number of HT data frames that were received at MCS 4.
RxFramesMCS5
This attribute shows the number of HT data frames that were received at MCS 5.
RxFramesMCS6
This attribute shows the number of HT data frames that were received at MCS 6.
RxFramesMCS7
This attribute shows the number of HT data frames that were received at MCS 7.
RxFramesMCS8
This attribute shows the number of data frames that were received at MCS 8.
RxFramesMCS9
This attribute shows the number of HT data frames that were received at MCS 9.
RxFramesMCS10
This attribute shows the number of HT data frames that were received at MCS 10.
RxFramesMCS11
This attribute shows the number of HT data frames that were received at MCS 11.
RxFramesMCS12
This attribute shows the number of HT data frames that were received at MCS 12.
RxFramesMCS13
This attribute shows the number of HT data frames that were received at MCS 13.
RxFramesMCS14
This attribute shows the number of HT data frames that were received at MCS 14.
RxFramesMCS15
This attribute shows the number of HT data frames that were received at MCS 15.
RxFramesMCS16
This attribute shows the number of HT data frames that were received at MCS 16.
RxFramesMCS17
This attribute shows the number of HT data frames that were received at MCS 17.
RxFramesMCS18
This attribute shows the number of HT data frames that were received at MCS 18.
RxFramesMCS19
This attribute shows the number of HT data frames that were received at MCS 19.
RxFramesMCS20
This attribute shows the number of HT data frames that were received at MCS 20.
RxFramesMCS21
This attribute shows the number of HT data frames that were received at MCS 21.
RxFramesMCS22
This attribute shows the number of HT data frames that were received at MCS 22.
RxFramesMCS23
This attribute shows the number of HT data frames that were received at MCS 23.
TxFramesMCS0
This attribute shows the number of HT data frames that were transmitted at MCS 0.
TxFramesMCS1
This attribute shows the number of HT data frames that were transmitted at MCS 1.
TxFramesMCS2
This attribute shows the number of HT data frames that were transmitted at MCS 2.
TxFramesMCS3
This attribute shows the number of HT data frames that were transmitted at MCS 3.
TxFramesMCS4
This attribute shows the number of HT data frames that were transmitted at MCS 4.
TxFramesMCS5
This attribute shows the number of HT data frames that were transmitted at MCS 5.
TxFramesMCS6
This attribute shows the number of HT data frames that were transmitted at MCS 6.
TxFramesMCS7
This attribute shows the number of HT data frames that were transmitted at MCS 7.
TxFramesMCS8
This attribute shows the number of data frames that were transmitted at MCS 8.
TxFramesMCS9
This attribute shows the number of HT data frames that were transmitted at MCS 9.
TxFramesMCS10
This attribute shows the number of HT data frames that were transmitted at MCS 10.
TxFramesMCS11
This attribute shows the number of HT data frames that were transmitted at MCS 11.
TxFramesMCS12
This attribute shows the number of HT data frames that were transmitted at MCS 12.
TxFramesMCS13
This attribute shows the number of HT data frames that were transmitted at MCS 13.
TxFramesMCS14
This attribute shows the number of HT data frames that were transmitted at MCS 14.
TxFramesMCS15
This attribute shows the number of HT data frames that were transmitted at MCS 15.
TxFramesMCS16
This attribute shows the number of HT data frames that were transmitted at MCS 16.
TxFramesMCS17
This attribute shows the number of HT data frames that were transmitted at MCS 17.
TxFramesMCS18
This attribute shows the number of HT data frames that were transmitted at MCS 18.
TxFramesMCS19
This attribute shows the number of HT data frames that were transmitted at MCS 19.
TxFramesMCS20
This attribute shows the number of HT data frames that were transmitted at MCS 20.
TxFramesMCS21
This attribute shows the number of HT data frames that were transmitted at MCS 21.
TxFramesMCS22
This attribute shows the number of HT data frames that were transmitted at MCS 22.
TxFramesMCS23
This attribute shows the number of HT data frames that were transmitted at MCS 23.
RxBandwidth
This attribute shows the bandwidth the access point used with the last received frame: 20 MHz (1) or 40 MHz (2).
RxGuardInterval
This attribute shows the length of the guard interval the WLAN bridge link used with last received frame: long (1) or short (2).
TxBandwidth
This attribute shows the bandwidth the WLAN bridge link used for transmitting the last frame: 20 MHz (1) or 40 MHz (2).
TxGuardInterval
This attribute shows the length of the guard interval the WLAN bridge link used for transmitting the last frame: long (1) or short (2).

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH